{"text_format":"3","workbook":"xls","n_sheets":11,"sheets":["汇总","材料检测","安全机械、材料检测","主体结构检测","钢结构检测","电气及设备工程检测","建筑节能及绿色建筑检测","玻璃门窗工程检测","室内空气检测","消防设施检测","工程监测"],"not_rendered":{"external_links":1,"defined_names":13},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"汇总","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"merged":[[0,0,0,4],[2,3,12,3],[2,4,12,4]],"flags":["formulas_cached_only"]}
["广东省医学科学院建设项目第三方检测监测服务项目工程量清单"]
["序号","检测项目","（审核）含税金额最高限（元）","投标下浮率（%）\n（综合单价及总价的下浮率，不得低于40%，低于40%为无效报价）","投标总价（元）\n（投标总价=2787772.80(1-投标下浮率)，不得高于167.27万元，高于167.27万元为无效报价）"]
[1,"材料检测",{"v":376800,"d":"376800.00"},"请填写","请填写"]
["2","安全机械及材料检测",{"v":212600,"d":"212600.00"}]
[3,"主体结构检测",{"v":281750,"d":"281750.00"}]
["4","钢结构检测",{"v":50000,"d":"50000.00"}]
["5","电气及设备工程检测",{"v":500125.7,"d":"500125.70"}]
["6","建筑节能及绿色建筑检测",{"v":413760,"d":"413760.00"}]
["7","玻璃门窗工程检测",{"v":209600,"d":"209600.00"}]
["8","室内空气检测",{"v":272000,"d":"272000.00"}]
["9","消防设施检测",75434.26]
["10","工程监测",{"v":395702.83999999997,"d":"395702.84"}]
["11","合计",{"v":2787772.8,"d":"2787772.80"}]

{"sheet":"材料检测","index":1,"n_rows":297,"n_cols":8,"rows_kept":297,"merged":[[0,0,0,7],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[3,1,6,1],[7,1,11,1],[12,1,17,1],[18,1,24,1],[25,1,32,1],[40,1,44,1],[46,1,47,1],[48,1,50,1],[51,1,53,1],[54,1,57,1],[54,5,55,5],[54,6,55,6],[54,7,55,7],[61,1,62,1],[66,1,71,1],[72,1,75,1],[76,1,82,1],[76,3,78,3],[76,4,78,4],[76,5,78,5],[76,6,78,6],[76,7,78,7],[83,1,86,1],[87,1,92,1],[87,3,88,3],[87,4,88,4],[87,5,88,5],[87,6,88,6],[87,7,88,7],[93,1,95,1],[96,1,97,1],[98,1,101,1],[102,1,106,1],[107,1,112,1],[107,7,108,7],[113,1,116,1],[117,1,119,1],[120,1,122,1],[123,1,125,1],[126,1,127,1],[128,1,132,1],[133,1,136,1],[133,4,135,4],[133,5,135,5],[133,6,135,6],[133,7,135,7],[137,1,142,1],[137,5,138,5],[137,6,138,6],[137,7,138,7],[143,1,144,1],[145,1,148,1],[149,1,154,1],[155,1,161,1],[162,1,165,1],[166,1,167,1],[168,1,171,1],[172,1,173,1],[174,1,176,1],[177,1,178,1],[179,1,182,1],[183,1,186,1],[187,1,189,1],[190,1,195,1],[191,5,192,5],[191,6,192,6],[191,7,192,7],[196,1,199,1],[197,5,198,5],[197,6,198,6],[197,7,198,7],[200,1,206,1],[202,5,203,5],[202,6,203,6],[202,7,203,7],[207,1,212,1],[208,5,209,5],[208,6,209,6],[208,7,209,7],[213,1,215,1],[216,1,217,1],[218,1,220,1],[221,1,224,1],[225,1,229,1],[230,1,233,1],[234,1,237,1],[235,5,236,5],[235,6,236,6],[235,7,236,7],[238,1,243,1],[244,1,249,1],[247,5,248,5],[247,6,248,6],[247,7,248,7],[250,1,252,1],[253,1,257,1],[258,1,262,1],[263,1,268,1],[269,1,270,1],[271,1,272,1],[273,1,275,1],[276,1,277,1],[278,1,279,1],[280,1,281,1],[282,1,284,1],[285,1,288,1],[290,1,295,1],[296,0,296,4]],"flags":["formulas_cached_only"]}
["材料检测清单"]
["序号","检测产品/对象","检测项目/参数","单位","数量\n（暂估）","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"水泥","胶砂强度","组",5,{"v":400,"d":"400.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.1.5"]
[2,null,"凝结时间","组",5,{"v":100,"d":"100.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.1.1"]
[3,null,"安定性","组",5,{"v":100,"d":"100.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.1.3"]
[4,null,"氯离子","组",5,{"v":300,"d":"300.00"},{"v":1500,"d":"1500.00"},"粤建检协[2015]8号4.1.23"]
[5,"砂","表观密度","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.4.2"]
[6,null,"颗粒级配","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.4.1"]
[7,null,"含泥量","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.4.8"]
[8,null,"泥块含量","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.4.9"]
[9,null,"氯离子","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.4.15"]
[10,"碎石","表观密度","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.5.2"]
[11,null,"颗粒级配","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.5.1"]
[12,null,"含泥量","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.5.8"]
[13,null,"泥块含量","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.5.9"]
[14,null,"坚固性","组",2,{"v":800,"d":"800.00"},{"v":1600,"d":"1600.00"},"粤建检协[2015]8号4.5.10"]
[15,null,"压碎指标","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.5.12"]
[16,"粉煤灰","需水量比","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.13.5"]
[17,null,"烧失量","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.13.9"]
[18,null,"三氧化硫","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.13.10"]
[19,null,"碱含量","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.13.13"]
[20,null,"含水量","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.13.4"]
[21,null,"安定性","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.13.7"]
[22,null,"游离氧化钙","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.13.12"]
[23,"外加剂","减水率","组",1,{"v":200,"d":"200.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.11.15"]
[24,null,"泌水率比","组",1,{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.11.16"]
[25,null,"抗压强度比","组",1,{"v":800,"d":"800.00"},{"v":800,"d":"800.00"},"粤建检协[2015]8号4.11.19"]
[26,null,"含气量","组",1,{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.11.21"]
[27,null,"含固量或含水率","组",1,{"v":150,"d":"150.00"},{"v":150,"d":"150.00"},"粤建检协[2015]8号4.11.6"]
[28,null,"氯离子含量","组",1,{"v":300,"d":"300.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.11.7"]
[29,null,"总碱量","组",1,{"v":300,"d":"300.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.11.10"]
[30,null,"硫酸钠","组",1,{"v":300,"d":"300.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.11.13"]
[31,"混凝土配合比","配合比设计/验证","组",5,{"v":1000,"d":"1000.00"},{"v":5000,"d":"5000.00"},"粤建检协[2015]8号4.8.9"]
[32,"预拌混凝土氯离子","氯离子含量","组",5,{"v":3000,"d":"3000.00"},{"v":15000,"d":"15000.00"},"粤建检协[2015]8号4.8.24"]
[33,"硬化混凝土氯离子含量","氯离子含量","组",5,{"v":1000,"d":"1000.00"},{"v":5000,"d":"5000.00"},"粤建检协[2015]8号4.8.23"]
[34,"混凝土试块","抗压强度","组",280,{"v":60,"d":"60.00"},{"v":16800,"d":"16800.00"},"粤建检协[2015]8号4.8.10"]
[35,"混凝土抗渗","抗渗等级","组",30,{"v":500,"d":"500.00"},{"v":15000,"d":"15000.00"},"粤建检协[2015]8号4.8.19"]
[36,"砂浆试块","抗压强度","组",20,{"v":50,"d":"50.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.9.10"]
[37,"水泥净浆试块抗压","抗压强度","组",8,{"v":50,"d":"50.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.9.10"]
[38,"钢筋原材","屈服强度、抗拉强度、断后伸长率、弯曲","组",80,{"v":150,"d":"150.00"},{"v":12000,"d":"12000.00"},"粤建检协[2015]8号4.16.1"]
[39,null,"重量偏差","组",80,{"v":50,"d":"50.00"},{"v":4000,"d":"4000.00"},"粤建检协[2015]8号4.16.2"]
[40,null,"强屈比、超强比","组",80,{"v":50,"d":"50.00"},{"v":4000,"d":"4000.00"},"粤建检协[2015]8号4.16.3"]
[41,null,"最大力总伸长率","组",80,{"v":50,"d":"50.00"},{"v":4000,"d":"4000.00"},"粤建检协[2015]8号4.16.4"]
[42,null,"反向弯曲","组",80,{"v":80,"d":"80.00"},{"v":6400,"d":"6400.00"},"粤建检协[2015]8号4.16.6"]
[43,"钢筋焊接","抗拉强度","组",30,{"v":100,"d":"100.00"},{"v":3000,"d":"3000.00"},"粤建检协[2015]8号4.17.1"]
[44,"机械连接","抗拉强度","组",50,{"v":100,"d":"100.00"},{"v":5000,"d":"5000.00"},"粤建检协[2015]8号4.18.1"]
[45,null,"残余变形","组",5,{"v":500,"d":"500.00"},{"v":2500,"d":"2500.00"},"粤建检协[2015]8号4.18.4"]
[46,"钢筋焊接网","拉伸","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.17.1、4.17.2"]
[47,null,"弯曲","组",2,{"v":80,"d":"80.00"},{"v":160,"d":"160.00"},"粤建检协[2015]8号4.17.3"]
[48,null,"剪切力","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.17.6"]
[49,"钢材原材","拉伸、弯曲","组",5,{"v":150,"d":"150.00"},{"v":750,"d":"750.00"},"粤建检协[2015]8号4.16.1"]
[50,null,"冲击试验","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.16.5"]
[51,null,"Z向性能","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.16.8"]
[52,"焊接材料","直径","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.31.1"]
[53,null,"长度尺寸偏差","组",2]
[54,null,"偏心(不圆)度","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.31.2"]
[55,null,"熔敷金属拉伸试验","组",2,{"v":1200,"d":"1200.00"},{"v":2400,"d":"2400.00"},"粤建检协[2015]8号4.31.3"]
[56,"钢管圆管","屈服强度、抗拉强度、断后伸长率、弯曲","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.25.3"]
[57,"钢材化学分析","C、Si、Mn、 P、S","组",2,{"v":1500,"d":"1500.00"},{"v":3000,"d":"3000.00"},"粤建检协[2015]8号4.16.9"]
[58,"镀锌钢板","镀锌层含量/厚度","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.25.7"]
[59,"普通螺栓","拉力试验","组",2,{"v":1800,"d":"1800.00"},{"v":3600,"d":"3600.00"},"粤建检协[2015]8号4.20.2"]
[60,null,"剪切试验","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.20.7"]
[61,"大六角高强螺栓","扭矩系数","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.19.5"]
[62,"扭剪型高强度螺栓","紧固轴力","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.19.6"]
[63,"高强度螺栓连接摩擦面","抗滑移系数","组",2,{"v":1200,"d":"1200.00"},{"v":2400,"d":"2400.00"},"粤建检协[2015]8号4.19.7"]
[64,"钢结构防腐涂料","在容器中状态","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.35.24"]
[65,null,"干燥时间（表干）","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.35.7"]
[66,null,"涂膜外观","组",2,{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},"粤建检协[2015]8号4.35.28"]
[67,null,"施工性","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.35.26"]
[68,null,"附着力","组",2,{"v":250,"d":"250.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.35.5"]
[69,null,"不挥发物中锌含量","组",2,{"v":800,"d":"800.00"},{"v":1600,"d":"1600.00"},"市场价"]
[70,"钢结构防火涂料","容器中状态","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.35.24"]
[71,null,"粘结强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.35.14"]
[72,null,"初期干燥抗裂性","组",2,{"v":250,"d":"250.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.35.2"]
[73,null,"抗压强度（非膨胀型检）","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.35.8"]
[74,"粘钢胶/浸渍胶","抗拉强度","组",2,{"v":1300,"d":"1,300.00"},{"v":2600,"d":"2600.00"},"粤建检协[2015]8号4.36.2、4.36.3"]
[75,null,"弹性模量"]
[76,null,"伸长率"]
[77,null,"抗压强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.36.5"]
[78,null,"抗弯强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.36.4"]
[79,null,"钢-钢拉伸剪切强度标准值","组",2,{"v":1000,"d":"1,000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.36.6"]
[80,null,"钢对C45混凝土拉伸粘结强度","组",2,{"v":1000,"d":"1,000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.36.8"]
[81,"锚固胶/植筋胶","抗压强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.36.5"]
[82,null,"抗弯强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.36.4"]
[83,null,"劈裂抗拉强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.36.1"]
[84,null,"钢-钢拉伸剪切强度标准值","组",2,{"v":1000,"d":"1,000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.36.6"]
[85,"碳纤维布","拉伸强度","组",2,{"v":1500,"d":"1,500.00"},{"v":3000,"d":"3000.00"},"粤建检协[2015]8号4.33.1"]
[86,null,"伸长率"]
[87,null,"弹性模量","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.33.2"]
[88,null,"纤维复合材与基材正拉粘结强度","组",2,{"v":1000,"d":"1,000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.33.4"]
[89,null,"单位面积质量","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.33.6"]
[90,null,"K数","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.33.8"]
[91,"蒸压加气混凝土砌块","抗压强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.27.8"]
[92,null,"干体积密度","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.27.11"]
[93,null,"导热系数","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.27.13"]
[94,"砌墙砖","抗压强度","组",1,{"v":300,"d":"300.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.26.4"]
[95,null,"密度","组",1,{"v":200,"d":"200.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.26.6"]
[96,"预拌砂浆","稠度","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.9.2"]
[97,null,"抗压强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.9.10"]
[98,null,"保水率","组",2,{"v":400,"d":"400.00"},{"v":800,"d":"800.00"},"粤建检协[2015]8号4.9.25"]
[99,null,"14d拉伸粘结强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.9.19"]
[100,"聚合物水泥砂浆","凝结时间","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.9.6"]
[101,null,"抗渗压力","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.9.22"]
[102,null,"抗压强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.9.10"]
[103,null,"抗折强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.9.17"]
[104,null,"粘结强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.9.18"]
[105,"防水卷材","纵横向拉力","组",3,{"v":300,"d":"300.00"},{"v":900,"d":"900.00"},"粤建检协[2015]8号4.38.5"]
[106,null,"伸长率","组",3,{"v":400,"d":"400.00"},{"v":1200,"d":"1200.00"}]
[107,null,"钉杆撕裂强度","组",3,{"v":300,"d":"300.00"},{"v":900,"d":"900.00"},"粤建检协[2015]8号4.38.6"]
[108,null,"耐热性","组",3,{"v":300,"d":"300.00"},{"v":900,"d":"900.00"},"粤建检协[2015]8号4.38.4"]
[109,null,"低温柔性","组",3,{"v":300,"d":"300.00"},{"v":900,"d":"900.00"},"粤建检协[2015]8号4.38.7"]
[110,null,"不透水性","组",3,{"v":300,"d":"300.00"},{"v":900,"d":"900.00"},"粤建检协[2015]8号4.38.3"]
[111,"聚合物水泥防水涂料","固体含量","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.40.2"]
[112,null,"拉伸强度、伸长率","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.40.5"]
[113,null,"不透水性","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.40.9"]
[114,null,"粘结强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.40.6"]
[115,"聚氨酯防水涂料","固体含量","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.40.2"]
[116,null,"拉伸强度、伸长率","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.40.5"]
[117,null,"不透水性","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.40.9"]
[118,"陶粒","颗粒级配","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.6.1"]
[119,null,"筒压强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.6.11"]
[120,null,"吸水率","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.6.5"]
[121,"挤塑板","表观密度","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.52.1"]
[122,null,"压缩强度","组",2,{"v":400,"d":"400.00"},{"v":800,"d":"800.00"},"粤建检协[2015]8号4.52.2"]
[123,null,"导热系数","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.52.3"]
[124,"镀锌电焊网","焊点抗拉","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.29.16"]
[125,null,"硫酸铜试验（镀锌层均匀性）","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.29.17"]
[126,"铝合金型材","壁厚","组",4,{"v":100,"d":"100.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.29.4"]
[127,null,"膜厚","组",4,{"v":200,"d":"200.00"},{"v":800,"d":"800.00"},"粤建检协[2015]8号4.29.5"]
[128,null,"漆膜硬度","组",4,{"v":200,"d":"200.00"},{"v":800,"d":"800.00"},"粤建检协[2015]8号4.29.15"]
[129,null,"附着性","组",4,{"v":300,"d":"300.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.29.14"]
[130,null,"抗拉强度、伸长率","组",4,{"v":500,"d":"500.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.29.2"]
[131,"防静电地板","均布荷载","组",1,{"v":1000,"d":"1000.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.59.7"]
[132,null,"集中荷载","组"]
[133,null,"极限集中荷载","组"]
[134,null,"防静电活动地板对地电阻","组",1,{"v":800,"d":"800.00"},{"v":800,"d":"800.00"},"市场价"]
[135,"陶瓷砖","尺寸偏差","组",6,{"v":300,"d":"300.00"},{"v":1800,"d":"1800.00"},"粤建检协[2015]8号4.15.1"]
[136,null,"表面质量","组",6]
[137,null,"吸水率","组",6,{"v":300,"d":"300.00"},{"v":1800,"d":"1800.00"},"粤建检协[2015]8号4.15.2"]
[138,null,"破坏强度","组",6,{"v":400,"d":"400.00"},{"v":2400,"d":"2400.00"},"粤建检协[2015]8号4.15.3"]
[139,null,"断裂模数","组",6,{"v":200,"d":"200.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.15.4"]
[140,null,"釉面抗龟裂","组",6,{"v":500,"d":"500.00"},{"v":3000,"d":"3000.00"},"粤建检协[2015]8号4.15.6"]
[141,"陶瓷砖胶粘剂","拉伸胶粘原强度","组",1,{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.37.17"]
[142,null,"晾置时间≥20min拉伸胶粘强度","组",1,{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.37.23"]
[143,"石材","吸水率","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.34.4"]
[144,null,"体积密度","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.34.3"]
[145,null,"压缩强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.34.1"]
[146,null,"弯曲强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.34.2"]
[147,"内外墙涂料","容器中状态","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.35.24"]
[148,null,"施工性","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.35.26"]
[149,null,"涂膜外观","组",2,{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},"粤建检协[2015]8号4.35.28"]
[150,null,"粘结强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.35.14"]
[151,null,"耐洗刷性","组",2,{"v":250,"d":"250.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.35.20"]
[152,null,"耐碱性","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.35.15"]
[153,"腻子","容器中状态","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.35.24"]
[154,null,"施工性","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.35.26"]
[155,null,"干燥时间（表干）","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.35.7"]
[156,null,"耐水性","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.35.17"]
[157,null,"耐碱性","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.35.15"]
[158,null,"打磨性","组",2,{"v":250,"d":"250.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.35.4"]
[159,null,"粘结强度（标准状态）","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.35.14"]
[160,"铝单板","涂层厚度","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.29.5"]
[161,null,"漆膜硬度","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.29.15"]
[162,null,"附着性","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.29.14"]
[163,null,"抗拉强度、伸长率","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.29.2"]
[164,"轻钢龙骨","壁厚","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.30.2"]
[165,null,"双面镀锌层厚度","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.30.4"]
[166,"石膏板","面密度","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.28.3"]
[167,null,"断裂荷载","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.28.10"]
[168,null,"表面吸水量","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.28.4"]
[169,null,"抗冲击性","组",2,{"v":600,"d":"600.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.28.13"]
[170,"岩棉/玻璃棉","导热系数","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.51.3"]
[171,null,"密度","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.51.6"]
[172,"橡塑棉","表观密度","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.52.1"]
[173,null,"导热系数","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.52.3"]
[174,null,"真空吸水率","组",2,{"v":400,"d":"400.00"},{"v":800,"d":"800.00"},"粤建检协[2015]8号4.52.8"]
[175,"井盖/箅子","承载能力","组",2,{"v":900,"d":"900.00"},{"v":1800,"d":"1800.00"},"粤建检协[2015]8号10.16.1"]
[176,null,"残余变形","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号10.16.2"]
[177,"双壁波纹管","环刚度","组",2,{"v":600,"d":"600.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号10.17.2"]
[178,null,"环柔性","组",2,{"v":400,"d":"400.00"},{"v":800,"d":"800.00"},"粤建检协[2015]8号4.43.10"]
[179,null,"烘箱试验","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.43.12"]
[180,null,"冲击性能","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.43.6"]
[181,"钢丝网骨架PE塑料复合管","外观","组",2,{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},"粤建检协[2015]8号4.44.1"]
[182,null,"平均外径","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.44.2"]
[183,null,"受压开裂稳定性","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.44.10"]
[184,null,"短期静液压强度","组",2,{"v":600,"d":"600.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.44.3"]
[185,"钢塑复合管（衬塑）","外观","组",2,{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},"粤建检协[2015]8号4.44.1"]
[186,null,"内衬塑料厚度","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.44.2"]
[187,null,"弯曲性能或压扁性能","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.44.5"]
[188,"冷热水用PP-R管材","外观","组",3,{"v":50,"d":"50.00"},{"v":150,"d":"150.00"},"粤建检协[2015]8号4.43.1"]
[189,null,"平均外径","组",3,{"v":100,"d":"100.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.43.2"]
[190,null,"壁厚","组",3]
[191,null,"纵向回缩率","组",3,{"v":200,"d":"200.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.43.8"]
[192,null,"简支梁冲击","组",3,{"v":200,"d":"200.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.43.7"]
[193,null,"静液压试验","组",3,{"v":1000,"d":"1000.00"},{"v":3000,"d":"3000.00"},"粤建检协[2015]8号4.43.13"]
[194,"冷热水用PP-R管件","外观","组",2,{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},"粤建检协[2015]8号4.43.1"]
[195,null,"承口平均内径","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.43.2"]
[196,null,"最小承口深度","组",2]
[197,null,"静液压试验","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.43.13"]
[198,"PVC-U排水管材","外观","组",3,{"v":50,"d":"50.00"},{"v":150,"d":"150.00"},"粤建检协[2015]8号4.43.1"]
[199,null,"平均外径","组",3,{"v":100,"d":"100.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.43.2"]
[200,null,"拉伸屈服应力","组",3,{"v":400,"d":"400.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.43.3"]
[201,null,"断裂伸长率","组",3]
[202,null,"维卡软化温度","组",3,{"v":250,"d":"250.00"},{"v":750,"d":"750.00"},"粤建检协[2015]8号4.43.4"]
[203,null,"落锤冲击","组",3,{"v":300,"d":"300.00"},{"v":900,"d":"900.00"},"粤建检协[2015]8号4.43.6"]
[204,null,"纵向回缩率","组",3,{"v":200,"d":"200.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.43.8"]
[205,"PVC-U排水管件","外观","组",2,{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},"粤建检协[2015]8号4.43.1"]
[206,null,"承口平均内径","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.43.2"]
[207,null,"最小承口深度","组",2]
[208,null,"维卡软化温度","组",2,{"v":250,"d":"250.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.43.4"]
[209,null,"烘箱试验","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.43.12"]
[210,null,"坠落试验","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.43.11"]
[211,"PVC-U 管道系统用塑料溶剂型胶粘剂","溶解性","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.37.3"]
[212,null,"粘度","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.37.6"]
[213,null,"粘结强度","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.37.8"]
[214,"阀门","壳体强度试验","组",3,{"v":400,"d":"400.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.54.2"]
[215,null,"密封试验","组",3,{"v":400,"d":"400.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.54.1"]
[216,"镀锌钢管","镀锌层表面质量","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.25.1"]
[217,null,"镀锌层的附着力","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.25.9"]
[218,null,"镀锌层均匀性","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.25.8"]
[219,"钢导线管","弯曲试验（外径≤25mm）","组",3,{"v":200,"d":"200.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.45.6"]
[220,null,"耐腐蚀性试验","组",3,{"v":240,"d":"240.00"},{"v":720,"d":"720.00"},"市场价"]
[221,null,"压力试验","组",3,{"v":200,"d":"200.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.45.8"]
[222,null,"冲击试验","组",3,{"v":300,"d":"300.00"},{"v":900,"d":"900.00"},"粤建检协[2015]8号4.45.9"]
[223,"建筑用绝缘电工套管","外观","组",3,{"v":50,"d":"50.00"},{"v":150,"d":"150.00"},"粤建检协[2015]8号4.45.1"]
[224,null,"最小壁厚","组",3,{"v":100,"d":"100.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.45.4"]
[225,null,"弯曲性能（外径≤25mm）","组",3,{"v":200,"d":"200.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.45.6"]
[226,null,"冲击性能","组",3,{"v":300,"d":"300.00"},{"v":900,"d":"900.00"},"粤建检协[2015]8号4.45.9"]
[227,null,"绝缘强度","组",3,{"v":300,"d":"300.00"},{"v":900,"d":"900.00"},"粤建检协[2015]8号4.45.10"]
[228,"电缆桥架","外观","组",2,{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},"粤建检协[2015]8号4.46.1"]
[229,null,"涂层厚度","组",2,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},"粤建检协[2015]8号4.46.8"]
[230,null,"附着力","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.46.9"]
[231,null,"锌层均匀性","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.46.7"]
[232,"母线槽","温升","组",1,{"v":7000,"d":"7000.00"},{"v":7000,"d":"7000.00"},"粤建检协[2015]8号4.62.2"]
[233,null,"介电性能（绝缘电阻）","组",1,{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.62.3"]
[234,null,"介电性能(电气强度)","组",1]
[235,null,"防护等级","组",1,{"v":2400,"d":"2400.00"},{"v":2400,"d":"2400.00"},"市场价"]
[236,"电线电缆","结构尺寸检查(绝缘厚度、外径）","芯",10,{"v":80,"d":"80.00"},{"v":800,"d":"800.00"},"粤建检协[2015]8号4.55.2"]
[237,null,"导体检查（导体种类、导体直流电阻）","芯",10,{"v":150,"d":"150.00"},{"v":1500,"d":"1500.00"},"粤建检协[2015]8号4.55.6"]
[238,null,"电压试验","芯",10,{"v":150,"d":"150.00"},{"v":1500,"d":"1500.00"},"粤建检协[2015]8号4.55.8"]
[239,null,"绝缘电阻","芯",10,{"v":150,"d":"150.00"},{"v":1500,"d":"1500.00"},"粤建检协[2015]8号4.55.7"]
[240,null,"热延伸试验","组",2,{"v":400,"d":"400.00"},{"v":800,"d":"800.00"},"粤建检协[2015]8号4.55.5"]
[241,null,"绝缘层老化前机械性能","组",2,{"v":250,"d":"250.00"},{"v":500,"d":"500.00"},"粤建检协[2015]8号4.55.3"]
[242,"网络线","衰减/插入损耗IL","组",1,{"v":300,"d":"300.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.61.6"]
[243,null,"近端串音衰减NEXT","组",1,{"v":300,"d":"300.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.61.9"]
[244,null,"近端串音衰减功率和  PS NEXT","组",1,{"v":300,"d":"300.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.61.10"]
[245,null,"等电平远端串音衰减ELFEXT","组",1,{"v":300,"d":"300.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.61.14"]
[246,null,"等电平远端串音衰减和PS ELFEXT","组",1]
[247,null,"回波损耗RL","组",1,{"v":300,"d":"300.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.61.5"]
[248,"空气开关","介电性能","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.56.12"]
[249,null,"温升试验","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.56.6"]
[250,null,"时间-(过)电流特性试验","组",2,{"v":600,"d":"600.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.56.5"]
[251,"漏电开关","介电性能","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号4.56.12"]
[252,null,"温升试验","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.56.6"]
[253,null,"在剩余电流条件下，验证动作特性","组",2,{"v":600,"d":"600.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.56.4"]
[254,null,"验证试验装置在额定电压极限值时的动作性能","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.56.3"]
[255,null,"时间-(过)电流特性试验","组",2,{"v":600,"d":"600.00"},{"v":1200,"d":"1200.00"},"粤建检协[2015]8号4.56.5"]
[256,"开关面板","防触电保护","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.57.2"]
[257,null,"温升","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.57.4"]
[258,null,"耐潮","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.57.7"]
[259,null,"绝缘电阻","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.57.9"]
[260,null,"电气强度","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.58.11"]
[261,"插座","接地措施","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.57.3"]
[262,null,"防触电保护","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.57.2"]
[263,null,"温升","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号4.57.4"]
[264,null,"防潮","组",2,{"v":300,"d":"300.00"},{"v":600,"d":"600.00"},"粤建检协[2015]8号4.57.7"]
[265,null,"绝缘电阻","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.57.9"]
[266,null,"电气强度","组",2,{"v":150,"d":"150.00"},{"v":300,"d":"300.00"},"粤建检协[2015]8号4.58.11"]
[267,"灯具","电性能（输入功率、输入电流、灯功率、功率因素、谐波电流）","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.58.19"]
[268,null,"光色参数（显示指数、相关色温、色差异、色品坐标、初始光通量、灯具效能、灯具光输出比、灯具光效）","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.58.18"]
[269,"建筑材料燃烧性能","A级","组",2,{"v":2700,"d":"2700.00"},{"v":5400,"d":"5400.00"},"粤建检协[2015]8号4.66.1"]
[270,null,"B级","组",4,{"v":4900,"d":"4900.00"},{"v":19600,"d":"19600.00"},"粤建检协[2015]8号4.66.4"]
[271,"消防水带","试验压力","组",1,{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},"市场价"]
[272,null,"最小爆破压力","组",1,{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},"市场价"]
[273,null,"附着强度","组",1,{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},"市场价"]
[274,"室内消火栓","水压强度","组",1,{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},"市场价"]
[275,null,"密封性能","组",1,{"v":800,"d":"800.00"},{"v":800,"d":"800.00"},"市场价"]
[276,"消防水枪（仅直流水枪）","耐水压强度","组",1,{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},"市场价"]
[277,null,"密封性能","组",1,{"v":800,"d":"800.00"},{"v":800,"d":"800.00"},"市场价"]
[278,"洒水喷头","水压密封和耐水压强度性能","组",1,{"v":1600,"d":"1600.00"},{"v":1600,"d":"1600.00"},"市场价"]
[279,null,"静态动作温度","组",1,{"v":800,"d":"800.00"},{"v":800,"d":"800.00"},"市场价"]
[280,"应急照明与疏散指示系统","充、放电试验","组",1,{"v":640,"d":"640.00"},{"v":640,"d":"640.00"},"市场价"]
[281,null,"基本功能试验","组",1,{"v":640,"d":"640.00"},{"v":640,"d":"640.00"},"市场价"]
[282,null,"恒定湿热试验","组",1,{"v":640,"d":"640.00"},{"v":640,"d":"640.00"},"市场价"]
[283,"电线电缆燃烧性能","耐火性能","组",2,{"v":3000,"d":"3000.00"},{"v":6000,"d":"6000.00"},"粤建检协[2015]8号4.65.3"]
[284,null,"单根阻燃","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号4.65.1"]
[285,null,"低烟性能 \n(烟密度)","组",2,{"v":3000,"d":"3000.00"},{"v":6000,"d":"6000.00"},"粤建检协[2015]8号4.65.4"]
[286,null,"无卤性能","组",2,{"v":4000,"d":"4000.00"},{"v":8000,"d":"8000.00"},"市场价"]
[287,"建筑材料放射性","内照射指数、外照射指数","组",2,{"v":1200,"d":"1200.00"},{"v":2400,"d":"2400.00"},"粤建检协[2015]8号11.5.1"]
[288,"建筑材料有害物质含量","挥发性有机化合物","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号11.4.2"]
[289,null,"游离甲醛","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号11.4.7"]
[290,null,"苯、甲苯、乙苯和二甲苯总和","组",2,{"v":3200,"d":"3200.00"},{"v":6400,"d":"6400.00"},"粤建检协[2015]8号11.4.3、11.4.4、11.4.17"]
[291,null,"可溶性重金属（铅、镉、铬、汞）","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号11.4.6"]
[292,null,"氯乙烯单体","组",2,{"v":1000,"d":"1000.00"},{"v":2000,"d":"2000.00"},"粤建检协[2015]8号11.4.8"]
[293,null,"甲醛释放量","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号11.4.1"]
["合计（元）",{"$nulls":5},{"v":376800,"d":"376800.00"}]

{"sheet":"安全机械、材料检测","index":2,"n_rows":16,"n_cols":8,"rows_kept":16,"merged":[[0,0,0,7],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[15,0,15,4]],"flags":["formulas_cached_only"]}
["安全机械及材料检测清单"]
["序号","检测产品/对象","检测项目/参数","单位","数量\n（暂估）","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"密目式安全网","尺寸、网目密度、抗冲击性、抗贯穿性、阻燃性","组",4,2500,10000,"粤建检协[2015]8号文7.14.10、7.14.9、7.14.7、7.14.6、7.14.8"]
[2,"安全带","整体静态负荷、整体动态负荷 、整体滑落、零部件静态负荷 、零部件动态负荷、零部件机械性能、阻燃性能 、缓冲试验 、缓冲器和速差式自控器试验","组",4,11500,46000,"粤建检协[2015]8号文7.16.1、7.16.2、7.16.3、7.16.4、7.16.5、7.16.6、7.16.7、7.16.8、7.16.9"]
[3,"安全帽","高温、低温、浸水处理后冲击吸收性能、高温、低温、浸水处理后耐穿刺性能、侧向刚性","组",4,1300,5200,"粤建检协[2015]8号文7.15.1、7.15.2、7.15.9"]
[4,"钢管脚手架直角扣件","直角扣件","组",6,4800,28800,"粤建检协[2015]8号文7.10.1、7.10.2、7.10.3、7.10.4"]
[5,"钢管脚手架旋转扣件","旋转扣件","组",6,4000,24000,"粤建检协[2015]8号文7.10.1、7.10.2、7.10.3"]
[6,"钢管脚手架对接扣件","对接扣件","组",6,4000,24000,"粤建检协[2015]8号文7.10.1、7.10.2、7.10.3"]
[7,"一般结构用焊接钢管","屈服强度、抗拉强度、断后伸长率、弯曲、压扁","组",6,1000,6000,"粤建检协[2015]8号文4.25.3、4.25.4"]
[8,"直插轮扣式钢管脚手架","可调托撑抗压强度、可调底座抗压强度、连接盘内侧环焊缝抗剪强度、连接盘单侧抗剪强度、连接盘双侧抗剪强度、连接盘抗拉强度、连接盘抗弯强度","组（8个）",6,3200,19200,"粤建检协[2015]8号文7.12.1（一组8个）、7.12.2（一组8个）、7.12.3（一组8个）"]
[9,"高处作业吊篮","安装质量","组",10,2000,20000,"粤建检协[2015]8号文7.4.1"]
[10,"塔吊检测","安装质量","组",6,2400,14400,"粤建检协[2015]8号文7.1.1"]
[11,"施工电梯检测","安装质量","组",6,2100,12600,"粤建检协[2015]8号文7.2.1"]
[12,"电梯检测","电梯和自动扶梯监测系统功能检测","组",6,400,2400,"粤建检协[2015]8号文9.2.5"]
["合计（元）",{"$nulls":5},212600]

{"sheet":"主体结构检测","index":3,"n_rows":10,"n_cols":8,"rows_kept":10,"merged":[[0,0,0,7],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[3,1,5,1],[6,1,8,1],[9,1,9,4]],"flags":["formulas_cached_only"]}
["主体结构工程检测清单"]
["序号","检测产品/对象","检测项目/参数","单位","检测数量","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"结构实体检验","混凝土强度","测区",2590,{"v":60,"d":"60.00"},{"v":155400,"d":"155400.00"},"粤建检协[2015]8号文第2.4.1"]
[2,null,"保护层厚度","构件",16,{"v":500,"d":"500.00"},{"v":8000,"d":"8000.00"},"粤建检协[2015]8号文第2.2.1"]
[3,null,"楼板厚度检测","构件",13,{"v":150,"d":"150.00"},{"v":1950,"d":"1950.00"},"粤建检协[2015]8号文第2.2.3"]
[4,"结构加固检测","植筋抗拔试验","个",32,{"v":1200,"d":"1200.00"},{"v":38400,"d":"38400.00"},"粤建检协[2015]8号文第2.9.1"]
[5,null,"粘合钢板正拉粘结强度","组",14,{"v":3000,"d":"3000.00"},{"v":42000,"d":"42000.00"},"粤建检协[2015]8号文第2.8.1"]
[6,null,"碳纤维抗拔试验","组",12,{"v":3000,"d":"3000.00"},{"v":36000,"d":"36000.00"},"粤建检协[2015]8号文第2.7.1"]
[7,"总计",{"$nulls":4},{"v":281750,"d":"281750.00"}]

{"sheet":"钢结构检测","index":4,"n_rows":7,"n_cols":8,"rows_kept":7,"merged":[[0,0,0,7],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[6,1,6,3]],"flags":["formulas_cached_only"]}
["钢结构检测清单"]
["序号","检测产品/对象","检测项目/参数","单位","暂定数量","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"焊缝质量","超声波","米",200,{"v":150,"d":"150.00"},{"v":30000,"d":"30000.00"},"粤建检协[2015]8号文第2.17.1"]
[2,"涂层质量","防腐涂层厚度","构件",40,{"v":250,"d":"250.00"},{"v":10000,"d":"10000.00"},"粤建检协[2015]8号文第2.17.8"]
[3,"涂层质量","防火涂层厚度","构件",40,{"v":250,"d":"250.00"},{"v":10000,"d":"10000.00"},"粤建检协[2015]8号文第2.17.9"]
[4,"合计（元）",{"$nulls":4},{"v":50000,"d":"50000.00"}]

{"sheet":"电气及设备工程检测","index":5,"n_rows":21,"n_cols":8,"rows_kept":21,"merged":[[0,0,0,7],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[3,1,12,1],[13,1,18,1]],"flags":["formulas_cached_only"]}
["电气设备检测清单"]
["序号","检测产品/对象","检测项目/参数","单位","检测数量","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"配电与照明系统节能检测","照度","处",86,800,{"v":68800,"d":"68800.00"},"粤建检协[2015]8号文第8.1.19"]
[2,null,"照明功率密度","处",86,800,{"v":68800,"d":"68800.00"},"粤建检协[2015]8号文第8.1.28"]
[3,null,"照度均匀度","处",86,800,{"v":68800,"d":"68800.00"},"粤建检协[2015]8号文第8.1.20"]
[4,null,"显色指数","处",86,800,{"v":68800,"d":"68800.00"},"粤建检协[2015]8号文第8.1.23"]
[5,null,"电源质量(供电电压偏差)","系统",2,2000,{"v":4000,"d":"4000.00"},"粤建检协[2015]8号文第8.1.30"]
[6,null,"电源质量(三相电压不平衡度)","系统",2,2000,{"v":4000,"d":"4000.00"},"粤建检协[2015]8号文第8.1.33"]
[7,null,"电源质量(功率因数)","系统",2,2000,{"v":4000,"d":"4000.00"},"粤建检协[2015]8号文第8.1.34"]
[8,null,"电源质量(谐波电压)","系统",2,2000,{"v":4000,"d":"4000.00"},"粤建检协[2015]8号文第8.1.31"]
[9,null,"电源质量(谐波电流)","系统",2,2000,{"v":4000,"d":"4000.00"},"粤建检协[2015]8号文第8.1.32"]
[10,null,"三相照明配电干线各相负荷平衡性","系统",20,1900,{"v":38000,"d":"38000.00"},"粤建检协[2015]8号文第8.1.29"]
[11,"建筑电气工程","馈电线路绝缘电阻","回路",54,500,{"v":27000,"d":"27000.00"},"粤建检协[2015]8号第8.1.1"]
[12,null,"电气装置绝缘电阻","个",32,500,{"v":16000,"d":"16000.00"},"粤建检协[2015]8号第8.1.1"]
[13,null,"电气装置耐压试验","个",32,500,{"v":16000,"d":"16000.00"},"粤建检协[2015]8号第8.1.2"]
[14,null,"漏电保护开关动作特性试验","个",40,300,{"v":12000,"d":"12000.00"},"粤建检协[2015]8号第8.1.8"]
[15,null,"接地系统电阻测试（接地电阻、等电位联结导通电阻、过渡电阻）","点",58,300,{"v":17400,"d":"17400.00"},"粤建检协[2015]8号第8.1.5"]
[16,null,"插座接线正确性","个",32,300,{"v":9600,"d":"9600.00"},"粤建检协[2015]8号第8.1.14"]
[17,"防雷装置工程","接地装置、引下线、接闪器、接闪网格、等电位连接、电涌保护器（SPD）","平方米",34462.85,2,{"v":68925.7,"d":"68925.70"},"防雷检测粤价函[2004]409号"]
[18,"合计",{"$nulls":4},{"v":500125.7,"d":"500125.70"}]

{"sheet":"建筑节能及绿色建筑检测","index":6,"n_rows":32,"n_cols":8,"rows_kept":32,"merged":[[0,0,0,7],[1,0,2,0],[1,1,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[3,1,14,1],[15,1,20,1],[21,1,30,1],[31,1,31,3]],"flags":["formulas_cached_only"]}
["建筑节能、绿色建筑及环保工程检测清单"]
["序号","检测参数",null,"计量单位","数量","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"建筑围护结构节能检测","墙体保温材料导热系数","组",2,{"v":1600,"d":"1600.00"},{"v":3200,"d":"3200.00"},"粤建检协[2015]8号文第4.14.7"]
[2,null,"墙体保温材料密度","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号文第4.14.6"]
[3,null,"墙体保温材料抗压强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号文第4.14.10"]
[4,null,"太阳辐射吸收系数","组",2,{"v":3000,"d":"3000.00"},{"v":6000,"d":"6000.00"},"粤建检协[2015]8号文第6.6.5"]
[5,null,"节能构造抽芯","组",6,{"v":1200,"d":"1200.00"},{"v":7200,"d":"7200.00"},"粤建检协[2015]8号文第6.12.1"]
[6,null,"外墙传热系数","组",1,{"v":15000,"d":"15000.00"},{"v":15000,"d":"15000.00"},"粤建检协[2015]8号文第6.6.2"]
[7,null,"外窗玻璃光学热工性能","组",2,{"v":4800,"d":"4800.00"},{"v":9600,"d":"9600.00"},"粤建检协[2015]8号文第6.5.1-6.5.10"]
[8,null,"外窗中空玻璃露点","组",2,{"v":1200,"d":"1200.00"},{"v":2400,"d":"2400.00"},"粤建检协[2015]8号文第6.5.11"]
[9,null,"屋面保温材料导热系数","组",2,{"v":1600,"d":"1600.00"},{"v":3200,"d":"3200.00"},"粤建检协[2015]8号文第4.14.7"]
[10,null,"屋面保温材料密度","组",2,{"v":200,"d":"200.00"},{"v":400,"d":"400.00"},"粤建检协[2015]8号文第4.14.6"]
[11,null,"屋面保温材料压缩强度","组",2,{"v":500,"d":"500.00"},{"v":1000,"d":"1000.00"},"粤建检协[2015]8号文第4.14.10"]
[12,null,"屋面保温材料燃烧性能","组",2,{"v":4900,"d":"4900.00"},{"v":9800,"d":"9800.00"},"粤建检协[2015]8号文第4.66.4"]
[13,"通风与空调系统","系统总风量","系统",3,{"v":3600,"d":"3600.00"},{"v":10800,"d":"10800.00"},"粤建检协[2015]8号文第6.7.2"]
[14,null,"风口风量","系统/个","3个系统（18个风口）",{"v":970,"d":"970.00"},{"v":17460,"d":"17460.00"},"粤建检协[2015]8号文第6.7.1"]
[15,null,"风机单位风量耗功率","系统",3,{"v":4700,"d":"4700.00"},{"v":14100,"d":"14100.00"},"粤建检协[2015]8号文第6.7.3"]
[16,null,"风管漏风量及变形量","系统",3,{"v":6000,"d":"6000.00"},{"v":18000,"d":"18000.00"},"粤建检协[2015]8号文第6.7.4"]
[17,null,"室内温湿度","点",50,{"v":790,"d":"790.00"},{"v":39500,"d":"39500.00"},"粤建检协[2015]8号文第6.7.6"]
[18,null,"多联式空调系统带负荷效果检测","台",2,{"v":6000,"d":"6000.00"},{"v":12000,"d":"12000.00"},"粤建检协[2015]8号文第8.14.8"]
[19,null,"室外环境噪声","点.次",8,{"v":1400,"d":"1400.00"},{"v":11200,"d":"11200.00"},"粤建检协[2015]8号文第6.1.1"]
[20,null,"室内背景噪声检测","点",10,{"v":1400,"d":"1400.00"},{"v":14000,"d":"14000.00"},"粤建检协[2015]8号文第6.1.1"]
[21,null,"楼板撞击声隔声性能","间",2,{"v":14000,"d":"14000.00"},{"v":28000,"d":"28000.00"},"粤建检协[2015]8号文第6.1.5"]
[22,null,"空气声隔声性能（隔墙）","间",2,{"v":14000,"d":"14000.00"},{"v":28000,"d":"28000.00"},"粤建检协[2015]8号文第6.1.3"]
[23,null,"空气声隔声性能（楼板）","间",2,{"v":14000,"d":"14000.00"},{"v":28000,"d":"28000.00"},"粤建检协[2015]8号文第6.1.3"]
[24,null,"电磁辐射","点",20,{"v":2560,"d":"2560.00"},{"v":51200,"d":"51200.00"},"市场价"]
[25,null,"土壤渗透系数","处",2,{"v":3000,"d":"3000.00"},{"v":6000,"d":"6000.00"},"市场价"]
[26,null,"透水铺砖渗透系数","处",2,{"v":3000,"d":"3000.00"},{"v":6000,"d":"6000.00"},"市场价"]
[27,null,"建筑能效测评","m2",23000,"/",{"v":56000,"d":"56000.00"},"粤建检协[2015]8号文第6.19.1"]
[28,null,"水质检测","处",1,{"v":14300,"d":"14300.00"},{"v":14300,"d":"14300.00"},"粤建检协[2015]8号文第6.14.1-6.14.20"]
[29,"合计（元）",{"$nulls":4},{"v":413760,"d":"413760.00"}]

{"sheet":"玻璃门窗工程检测","index":7,"n_rows":17,"n_cols":8,"rows_kept":17,"merged":[[0,0,0,7],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[4,1,5,1],[7,1,11,1],[12,1,13,1],[16,1,16,2]],"flags":["formulas_cached_only"]}
["玻璃门窗检测清单"]
["序号","检测产品/对象","检测项目/参数","单位","暂定数量","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"铝合金窗\n（宽3m×3m以内）","气密性能、水密性能、抗风压性能","组",8,{"v":4000,"d":"4000.00"},{"v":32000,"d":"32000.00"},"粤建检协[2015]8号第5.2.1-5.2.3"]
[2,"硅酮耐候密封胶","密封胶胶相容性、剥离粘结性","组",8,{"v":4500,"d":"4500.00"},{"v":36000,"d":"36000.00"},"粤建检协[2015]8号第5.4.1、5.4.2"]
[3,null,"密封胶弹性恢复率、拉伸模量、定伸粘结性","组",8,{"v":4500,"d":"4500.00"},{"v":36000,"d":"36000.00"},"粤建检协[2015]8号第5.5.6-5.5.8"]
[4,"中空玻璃","密封性能","组",8,{"v":2000,"d":"2000.00"},{"v":16000,"d":"16000.00"},"粤建检协[2015]8号 第5.9.9"]
[5,"钢化玻璃","表面应力","组",8,{"v":600,"d":"600.00"},{"v":4800,"d":"4800.00"},"粤建检协[2015]8号第5.9.5"]
[6,null,"碎片状态","组",8,{"v":600,"d":"600.00"},{"v":4800,"d":"4800.00"},"粤建检协[2015]8号第5.9.4"]
[7,null,"抗冲击性","组",8,{"v":200,"d":"200.00"},{"v":1600,"d":"1600.00"},"粤建检协[2015]8号第5.9.6"]
[8,null,"霰弹袋冲击性能","组",8,{"v":300,"d":"300.00"},{"v":2400,"d":"2400.00"},"粤建检协[2015]8号第5.9.7"]
[9,null,"耐热冲击性能","组",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"粤建检协[2015]8号第5.9.6"]
[10,"护栏","抗水平荷载性能","组",1,{"v":10000,"d":"10000.00"},{"v":10000,"d":"10000.00"},"粤建检协[2015]8号第5.11.1"]
[11,null,"耐软重物撞击性能","组",1,{"v":10000,"d":"10000.00"},{"v":10000,"d":"10000.00"},"粤建检协[2015]8号第5.11.3"]
[12,"防火窗","耐火极限","组",2,{"v":11200,"d":"11200.00"},{"v":22400,"d":"22400.00"},"市场价"]
[13,"防火玻璃32厚","耐火极限","组",3,{"v":11200,"d":"11200.00"},{"v":33600,"d":"33600.00"},"市场价"]
[14,"总计",{"$nulls":4},{"v":209600,"d":"209600.00"}]

{"sheet":"室内空气检测","index":8,"n_rows":11,"n_cols":9,"rows_kept":11,"merged":[[0,0,0,8],[1,0,2,0],[1,1,2,1],[1,2,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[1,8,2,8],[3,1,9,1],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,0,10,6]],"flags":["formulas_cached_only"]}
["室内环境质量检测清单"]
["序号","项目","检测参数",null,"计量单位","检测数量","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"室内环境质量检测","氡气",null,"点",85,{"v":600,"d":"600.00"},{"v":51000,"d":"51000.00"},"11.1.2"]
[2,null,"甲醛",null,"点",85,{"v":600,"d":"600.00"},{"v":51000,"d":"51000.00"},"11.1.5"]
[3,null,"氨",null,"点",85,{"v":400,"d":"400.00"},{"v":34000,"d":"34000.00"},"11.1.6"]
[4,null,"苯",null,"点",85,{"v":400,"d":"400.00"},{"v":34000,"d":"34000.00"},"11.1.1"]
[5,null,"甲苯",null,"点",85,{"v":400,"d":"400.00"},{"v":34000,"d":"34000.00"},"11.1.3"]
[6,null,"二甲苯",null,"点",85,{"v":400,"d":"400.00"},{"v":34000,"d":"34000.00"},"11.1.4"]
[7,null,"TVOC",null,"点",85,{"v":400,"d":"400.00"},{"v":34000,"d":"34000.00"},"11.1.7"]
["合计（元）",{"$nulls":6},{"v":272000,"d":"272000.00"}]

{"sheet":"消防设施检测","index":9,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[0,0,0,6],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6]],"flags":["formulas_cached_only"]}
["消防设施检测清单"]
["序号","试验检测项目","暂定数量","单位","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"消防设施",37717.13,"㎡",{"v":2,"d":"2.00"},75434.26,"市场价"]

{"sheet":"工程监测","index":10,"n_rows":21,"n_cols":8,"rows_kept":21,"merged":[[0,0,0,7],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[3,1,7,1],[8,1,13,1],[15,1,16,1],[17,1,18,1]],"flags":["formulas_cached_only"]}
["监测清单"]
["序号","检测产品/对象","检测项目/参数","单位","检测数量","综合单价限价（元）","合价（元）","收费依据"]
[]
[1,"基坑监测点埋设费","高程基准点","点",3,{"v":250,"d":"250.00"},{"v":750,"d":"750.00"},"粤建检协(2015〕8号3.1.1-②"]
[2,null,"位移工作基点","点",2,{"v":3500,"d":"3500.00"},{"v":7000,"d":"7000.00"},"粤建检协(2015〕8号3.1.3-②"]
[3,null,"坡顶水平位移/竖向位移","点",11,{"v":250,"d":"250.00"},{"v":2750,"d":"2750.00"},"粤建检协(2015〕8号3.1.1-①、3.1.3-①"]
[4,null,"地下管线和周边建筑沉降","点",9,{"v":250,"d":"250.00"},{"v":2250,"d":"2250.00"},"粤建检协(2015〕8号3.1.1-①"]
[5,null,"地下水位","孔（6米）",7,{"v":1500,"d":"1500.00"},{"v":10500,"d":"10500.00"},"粤建检协(2015〕8号3.1.10-①②"]
[6,"基坑监测费","平面基准网点单测","点·次",18,{"v":2181,"d":"2181.00"},{"v":39258,"d":"39258.00"},"粤建检协(2015〕8号3.1.3-⑥二等单测简单"]
[7,null,"高程基准网点监测","点·次",18,{"v":1216,"d":"1216.00"},{"v":21888,"d":"21888.00"},"粤建检协(2015〕8号3.1.1-④二等单测简单"]
[8,null,"基坑坡顶水平位移","点·次",550,{"v":74,"d":"74.00"},{"v":40700,"d":"40700.00"},"粤建检协(2015〕8号3.1.3-④二等单向简单"]
[9,null,"基坑坡顶竖向位移","点·次",550,{"v":50,"d":"50.00"},{"v":27500,"d":"27500.00"},"粤建检协(2015〕8号3.1.1-③二等单测简单"]
[10,null,"地下管线和周边建筑沉降","点·次",450,{"v":50,"d":"50.00"},{"v":22500,"d":"22500.00"},"粤建检协(2015〕8号3.1.1-③二等单测简单"]
[11,null,"地下水位","点·次",350,{"v":200,"d":"200.00"},{"v":70000,"d":"70000.00"},"粤建检协(2015〕8号3.1.10-③"]
[12,"基坑技术费","技术费","项",1,"/",48806.12,"粤建检协(2015〕8号3.1"]
[13,"主体测点埋设费","高程基准点","点",3,{"v":250,"d":"250.00"},{"v":750,"d":"750.00"},"粤建检协(2015〕8号3.1.1-②"]
[14,null,"主体沉降监测点","点",92,{"v":250,"d":"250.00"},{"v":23000,"d":"23000.00"},"粤建检协(2015〕8号3.1.1-①"]
[15,"主体沉降监测费","高程基准网点监测","点·次",11,{"v":1216,"d":"1216.00"},{"v":13376,"d":"13376.00"},"粤建检协(2015〕8号3.1.1-④二等单测简单"]
[16,null,"主体沉降监测","点·次",1012,{"v":50,"d":"50.00"},{"v":50600,"d":"50600.00"},"粤建检协(2015〕8号3.1.1-③二等单测简单"]
[17,"主体沉降技术费","技术费","项",1,"/",14074.72,"粤建检协(2015〕8号3.1"]
[18,"合计",{"$nulls":4},{"v":395702.83999999997,"d":"395702.84"}]